{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["XX省（市、区）"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"XX省（市、区）","index":0,"n_rows":12,"n_cols":16,"rows_kept":12,"merged":[[11,0,11,15]],"flags":["formulas_cached_only"]}
["序号","企业名称","社会信用代码","机组编号","发电燃料类型","装机容量\n（MW）","机组类型","发电量\n（MWh)","供电量\n（MWh)","供热量（GJ）","供热比","冷却方式","拟分配配额\n吨CO2当量\n（方案一）","拟分配配额（方案一）","拟分配配额（方案一）","拟分配配额\n吨CO2当量\n（方案二）"]
[1,{"$nulls":12},"超超临界","空冷"]
[2,{"$nulls":12},"超临界","水冷"]
[3,{"$nulls":12},"亚临界"]
[4,{"$nulls":12},"高压超高压"]
[5,{"$nulls":12},"循环流化床"]
[6,{"$nulls":12},"燃气"]
[7,{"$nulls":12},"特殊燃料"]
[8]
[9]
["…"]
["注：\n1.已完成2018年度碳排放数据核查的省份采用经核查的数据，尚未完成的省份采用重点排放单位自行填报数据。\n2.供热比的计算方法如下。\n  (1) 对于燃煤热电联产机组（不含锅炉向外直供蒸汽），其供热比计算公式参考行业标准DL/T 904-2015 《火力发电厂技术经济指标计算方法》公式（147）进行计算。\n  (2) 对于既有锅炉抽蒸汽供热，又有汽轮机抽汽供热的情况，其供热比计算公式如下：\n锅炉主蒸汽抽汽外供热量为Q1，汽轮机热耗量为Qsr，汽轮机供热量为Qgr，则供热比计算公式为： \n此时机组的供热量为两部分供热量之和，即Q1+Qgr。\n  (3) 对于燃气热电联产机组，其供热比等于统计期内机组供热量与燃气产生的热量（燃气消耗量×燃气低位发热量）的百分比。\n"]